Deep-Sea Titanium Alloy Camera Housing
Can your sub-sea cameras withstand the harsh conditions of the marine environment? If not, upgrading the housing material is one of the options. By utilizing titanium housing, sub-sea cameras can reach ocean depths as great as 6000m.
Titanium housing construction can provide a reliable and robust protection for deep-sea equipment, like video cameras, recorder and optical data transmitters. This camera shell is usually made from Grade 5 titanium (Ti-6Al-4V), which is highly durable and corrosion-resistant, making it perfect as a housing material for underwater cameras .
Why choose us?
1. Using aerospace grade titanium as raw material
Our deep-sea camera housings are manufactured from high-grade titanium bar, which is a solid material manufactured according to AMS specifications. 
2. High dimensional accuracy and surface quality
Through integral CNC machining from titanium rod, the housings maintain consistent in mechanical properties and have no welds, this can prevent any potential leakage. The precision-machined sealing grooves allow every O-ring to seat perfectly, achieving optimal sealing performance to prevent leaks. This directly enhances subsea equipment’s durability and operational safety.
Quality Control System
As a AS 9100 & ISO 9001 certified factory, a full-process quality traceability system has been established from raw material warehousing to finished product delivery. Each housing is delivered with the following reports:
•Material Mill Certificate
•Non-Destructive Testing Report
•Pressure Test Certificate
•Dimensional Inspection Report
Deep-water applications include:
1. Seafloor mapping and imaging
2. Marine archaeology
3. Deep-water exploration
4. Defense and security
5. Sub-sea pipeline inspection
6. Offshore engineering  ...
Whether you are oceanographic institutes, offshore energy companies, or documentary filmmakers, our deep-sea titanium housing is not just a protective shell，it's a mission-critical platform for exploring the final frontier on Earth.
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